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	Product characteristics 

	(text highlighted in red can be deleted depending on your choice)

	

	Installation 

	Topfix Max: this product is installed onto a closed structure (e.g. a skylight)

	Topfix Max F: this product is installed onto an open structure

	Top-bottom and Bottom-Top (with additional supporting) installation is possible.

	The inclination angle may vary between 0° and 90°. The usage of a type of fabric is defined in function of the inclination angle.

	

	Head box 

	Dimensions: 260 mm height and 202 mm depth

	Profiles are made of extruded aluminium.

	The head box must always be supported:

	    - Depending on the inclination angle (0°-90° in case of the head box is positioned at the bottom), an external support bracket is supplied to prevent the head box from sliding out of the side guiding channels

	    - Depending on the inclination angle (45°-90° in case the head box is positioned on the top), an internal support bracket is provided in the head ox to prevent the fabric set from sliding out

	

	Side guiding channels 

	Are made of 2 extruded aluminum profiles.

	Dimensions :

	    - Side guiding channel: W 69.5 mm D 84.5 mm (only if Topfix Max)

	    - Side guiding channel: W 91 mm x D 84.5 mm (only if Topfix Max F)

	The side guiding channels are equipped with tracks on which the wheels of the trolleys of the bottom bar. This ensures a perfect movement guidance of the bottom bar.

	Topfix Max F: the side guiding channels are equipped with a hidden drainage gutter to ensure to drain away the rainwater which hits the fabric via the bottom bar and the side guiding channels

	Topfix Max F: those side guiding channels combined with the trolleys provide a level of mechanical security on the bottom bar

	Each side guiding channel has an integrated UPVC inner rail with a co-extruded, wear resistant top layer to ensure smooth and silent functioning.

	The HPVC inner rail is equipped with 2 S profiles on each side, to compensate heavy wind loads.

	

	Fabric tube 

	Made of galvanised steel.

	An integrated recessed fabric groove limits compression of the fabric loop.

	Is equipped with patented cone shaped fabric tube end pieces to compensate the thicker ends of the zipper.

	They also contain a belt disk to roll up the tension belt.

	You can disassemble the fabric set on the side of the removable profile of the head box; the left or right position is determined in this way (cable feed).

	

	Fabric 

	All fabrics consist of a single piece of fabric, except if the height is greater than the fabric tube width.

	The fabrics are confectionated horizontally.

	The vertical borders are equipped with a zipper to keep the fabric firmly (windproof) in the side guiding channel.

	The zipper is welded at high frequency, always on the least visible side.

	●  Polyester fabric (semi-transparent):

	    - Fire resistance: M1 (NFP 92503), B-s2d0 (Euroclass EN 13501-1)

	    - Weight: ± 380-420 g/m², thickness: 0.43-0.45 mm

	●  Polyester fabric (blackout) -> only applicable with Topfix Max:

	    - Fire resistance: M2 (NFP 92503), B-s2d0 (Euroclass EN 13501-1)

	    - Weight: ± 650 g/m², thickness: 0.60 mm

	●  Polyester fabric waterproof -> only applicable with Topfix Max F:

	    - Fire resistance: M2 (NFP 92503)

	    - Weight: ± 620 g/m², thickness: 0.56 mm

	

	

	

	Bottom bar 

	Is made of 1 extruded aluminium profile.

	Topfix Max F: a black HPVC leaf catcher has been provided in the bottom bar; that stops the dirt so the drainage channels do not get clogged

	

	Tension system 

	The system is tensioned using a permanently pretensioned Aramide/Kevlar-belt.

	

	Colour 

	All visible aluminium profiles (head box, side guiding channels and bottom bar): Powder coated (60-80 µm) in the same colour, as the external joinery.

	The side supporting end caps (cast aluminium): Powder coated (60-80 µm) in the same colour as the profiles.

	Extra pre-treatment Seaside Quality possible.

	

	Control 

	Electrical: by means of 230 V AC tubular motor or by 24 V DC tubular motor, without emergency manual control

	The motor connection is included in the sun protection category.

	UV resistant cable included.

	The electrical connection and all additional wiring are included in the electrical category.

	

	Warranty 

	10-year warranty on coatings on the aluminium profiles.

	5-year warranty on the windproof-technology:

	    - Zipper remains in side guiding channel

	    - Adhesion of zipper to fabric

	5-year warranty on defects arising from normal domestic use and regular maintenance.

	5-year warranty on the electronic control (Somfy automation).

	5-year warranty on the fabric collection.

	Every individual sun protection product can be identified afterwards and linked to a warranty number or a unique screen ID.

	This identification occurs via a QR code, which is placed within reach (without the use of tools) and easily scannable with a smartphone.

	The essential product details (dimensions, colours, type of fabric, motor type, etc.) can be consulted at any time.

	

	Wind class 

	⌂ Guaranteed up to 120 km/h in closed position (EN 13561:2004+A1:2008 conform wind class 3)*.

	    * Wind tunnel test report 'Von Karman Institute' (n° EAR0852 - 2009-07) (W 3,000 mm x P 3,000 mm)

	

	Standards and certificates 

	⌂ This product is manufactured in accordance with: EN 13561 and conforms to and/or has been tested in accordance with these standards

	References and certificates:

	    - Declaration of performance: DoP-201409-F006



