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	Product characteristics

	(text highlighted in red can be deleted depending on your choice)

	

	Installation 

	This product is installed in front of a curtain wall with fully finished head box -> Recessed or Surface-mounted.

	This patented solution is in sush way developped that you can link one screen after the other infinitely.

	The installation will always start with the 1st screen on the Left hand side.

	 - Installation method 7A (Standard, fabric close to the window)

	Necessary securing for head box width > 3,600 mm, in order to avoid bending

	The side supporting end caps of the head box, supporting the roll-up mechanism are equipped with pins, which connect the head box with the side guiding channels.

	Because of the adjustable pins the head box can easily be installed after the side guiding channels.

	During installation the fabric set will stay assambled in the head box.

	During installation, you have the flexibility to bring the cable upwards, downwards or to the backside of the head box. These possibilities depend on the fixation direction of the head box.

	

	Head box 

	Profiles are made of extruded aluminium.

	The side supporting end caps are made of cast aluminium.

	Head box design: Square (rectangular).

	Dimensions: 160 mm height and 110 mm depth.

	

	Side guiding channels 

	Composition:

	Are made of extruded aluminium profiles.

	 - Design guarantees central securing to the curtain wall

	    - Every side guiding channel is equipped with an powder coated base plate under 0° and made of cast aluminium

	 - Inner rail:

	    - Powder coated, aluminium

	    - Smooth-technology: coextruded, wear-resistant top layer (= Smooth and quiet, long-term durable operation, without additional maintenance)

	    - Neoprene buffer zones (= Compensate for gusts of wind and contribute to constant fabric tension)

	Installation :

	Fixed directly onto the frame/construction and then clicked together without screws.

	Side guiding channel option:

	 - C.50-coupling side guiding channel (standard): W 50 mm x D 58 mm, with standard removable profile

	 - C.50-coupling side guiding channel: W 50 mm x D 90 mm, with removable profile to host a power lead with plug and socket

	As an option a finishing profile for a nice slick finish of the coupling side guiding channel, where no inner rail is needed, is available.

	This finishing profile is mounted on the 1st screen(start)screen and on the last screen (width left & right).

	They are fixed in the middle of the curtain wall profile and screwless linked into each other.

	Each side guiding channel has an integrated aluminium inner rail, with a wear resistant UPVC finish. In this innerrail the fabric slides.

	The aluminium inner rail is equipped with Neoprene buffer zones to compensate heavy wind loads.

	

	Fabric set

	Composition:

	 - Fabric tube: Galvanised steel, with a recessed detail in which the removable UPVC insert clicks into place

	   (= Counteracts horizontal line formation by limiting the penetration of the fabric and facilitates (dis)assembly of the fabric)

	 - At motor side (always Rhs) a narrowed cone shaped fabric tube end piece, the motor slide and the electrical connection are installed

	 - At bearing side (always Lhs) a narrowed cone shaped fabric tube end piece and a bearing slide are installed

	 - The narrowed cone shaped fabric tube end pieces will compensate the bigger dimensions of the zipper

	Connect&Go-technology: (Dis)assembly of the fabric set is facilitated by means of the electrical connection: Connect&Go-technology.

	Click&Safe-technology: The fabric set can be clicked into the head box without screws so that the installer has his hands free to safely complete the installation.

	

	Fabric

	All fabrics consist of a single piece of fabric, except when the height is greater than the fabric tube width.

	Confection :

	 - Horizontally

	 - Fixscreen-technology: the vertical borders are equipped with a symmetrical zipper

	   (= This symmetrical shape ensures that the fabric absorbs the wind load well. As a result, the fabric is firmly affixed in both side guiding channels and remains windproof in any position) 

	 - Welding zipper: High-frequency, always on the least visible side. (= Durable and aesthetic adhesion of the zippers to the fabric)

	

	Applicable dimensions of fabrics, see brochure.

	Type of fabric :

	●  Fibre glass fabric (semi-transparent):

	    - Fire resistance: M1 (NFP 92503), C-s3d0 (Euroclass EN 13501-1)

	    - Weight: ± 520-620 g/m², thickness: 0.53-0.80 mm

	●  Fibre glass fabric (blackout):

	    - Fire resistance: M1 (NFP 92503)

	    - Weight: ± 660 g/m², thickness: 0.75 mm

	

	Weighted bottom bar

	Composition:

	 - Bottom bar: Extruded aluminium, solidly weighted with bars in galvanised steel. (= Facilitates the smooth guiding system and tension of the fabric)

	 - Ballast: Steel bar. The bar is covered with PE foam to prevent contact between the aluminium and steel and to buffer noise

	 - Dimensions bottom bar: H 35 mm x D 40 mm (excl. sealing strip)

	Finishing :

	 - The bottom bar disappears completely into the head box

	 - Welded seam hidden in the bottom bar

	 - Fitted with UPVC end pieces. Available in 4 colours: black, white, grey and cream

	 - Fitted with a UPVC sealing strip to close off the sill. Available in 2 colours: black and grey.

	 - Easy (dis)assembly of the fabric by a hidden UPVC click profile

	

	Colour

	Aluminum profiles (head box, side guiding channels and bottom bar): Powder coated (60-80 µm) or anodised (20 µm) in the same colour as the external joinery.

	Side supporting end caps (cast aluminium): Powder coated in the same colour as the profiles.

	In the case of anodised profiles (head box, side guiding channels and bottom bar), the side supporting end caps are powder coated in the most suitable colour (60-80 µm).

	

	Control

	Electric:

	 - 230 V AC tubular motor, without emergency manual control

	 - 230 V AC tubular motor, with obstacle detection (Detecto) and continuous fabric stretch compensation

	 - Mechanical motor isn't possible

	The motor connection is included in the sun protection category and is provided with a uv-resistant cable.

	The electrical connection and all additional wiring are included in the electrical category.

	

	Connect&Go-technology: electrical connection 

	Facilitates quick and easy (dis)assembly of the screen set.

	When installing the fabric set in the head box, the motor connector moves via the straight guiding system of the corresponding side supporting end piece in the cable connector; both connector clips are fixed into place and form a perfect electrical connection inside the head box.

	

	Renson Connect

	Optional control with Renson smartphone application for iOS and Android, including product details and product-specific tips & tricks in the app.

	

	Warranty and product information via QR code

	10-year warranty on coatings on the aluminium profiles.

	7-year warranty on electronic motors with obstacle detection (Detecto).

	7-year warranty on the windproof-technology:

	 - Zipper remains in side guiding channel

	 - Optimal adhesion of zipper to fabric

	5-year warranty on defects arising from normal domestic use and regular maintenance.

	5-year warranty on motors.

	5-year warranty on the fabric collection.

	Every individual sun protection product can be identified afterwards and linked to a warranty number or a unique screen ID.

	This identification is done thanks to a QR code, which is placed in an easily accessible location (can be consulted without using extra tools) and can be easily scanned using a smartphone or tablet.

	The essential product details (dimensions, colours, fabric type, motor type, etc.) can be consulted at any time.

	

	Wind class 

	This product meets European standard EN13561.

	Guaranteed up to 130 km/h in closed position (EN 13561:2004+A1:2008 in accordance with wind class 3). The wind resistance depends on the dimensions and is available upon request.

	Wind tunnel test report by ‘Velux’ (WTT17-001 Fixscreen Minimal MS7 S): wind resistance up to and including 130 km/h in closed position (tested on a 3200 mm x 3200 mm screen).

	

	Standards and certificates

	This product is manufactured in accordance with: EN 13561 and conforms to and/or has been tested in accordance with these standards.

	Declaration of performance: DoP-2016SC00006.

	AluEco en VMRG Sun protection certificate.



