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	Product characteristics

	(text highlighted in red can be deleted depending on your choice)

	

	Installation 

	This product is installed with fully finished head box:

	'Freestanding' F (cannot be coupled) without window behind it.

	 - Installation method 7A (Standard, inside patio cover or balcony)

	 - Installation method 7B (Outside patio cover or balcony)

	The side supporting end caps of the head box, which support the roller mechanism and are equipped with pins, connect the head box to the side guiding channels.

	One side supporting end cap is equipped with the cable connector of the electrical connection.

	During the installation of the fabric set (fabric tube + fabric + motor), the electrical connection is made easily via the motor connector.

	Connect&Go-technology: facilitates quick and easy (dis)assembly of the fabric set.

	The cable feed is equipped in the head box or is equipped in the side supporting end cap.

	You can disassemble the fabric set on the side of the removable profile of the head box; the left or right position is determined in this way (cable feed).

	

	Head box 

	Composition: extruded aluminium.

	Head box design: Square (rectangular).

	Dimensions: 150 mm height and 110 mm depth (max. surface 16.8 m²).

	Head box extension: possible up to 500 mm. Head box extension not possible in case of deep side guiding channel.

	

	Side guiding channels 

	Composition:

	 - Outer profiles: extruded aluminium

	 - 3-piece: u-profile allows for easy disassembly of the fabric set; without complete disassembly of the side guiding channel, without drilling or channelling, which guarantees water and wind proofing

	 - Inner rail:

	    - HPVC plastic (= robust design guarantees high wind guarantees)

	    - Smooth-technology: coextruded, wear-resistant top layer (= Smooth and quiet, long-term durable operation, without additional maintenance)

	    - Neoprene buffer zones (60 mm long) (= Compensate for gusts of wind and contribute to constant fabric tension)

	    - Flush-mounted in 3-piece side guiding channel, reducing visibility to 13.78 mm

	Side guiding channel option:

	 - Deep side guiding channel (standard): W 35 mm x D 110 mm, in 3 parts, u-profile; side guiding channel depth = head box depth, equipped with a base plate under 0° or 5° (only for method 7A) made of fibre glass-reinforced polyamide

	 - Deep side guiding channel (7B installation only): Possible with saw cut for application with balustrade

	 - Closed side guiding channel: W 35 mm x D 48 mm, in 3 parts; in case used with a self-designed removable finishing, equipped with a base plate under 0° or 5° (only for method 7A) made of fibre glass-reinforced polyamide

	 - Fixed directly onto the frame/construction. No screws are visible from the façade side

	

	Fabric set

	Composition:

	 - Fabric tube: Galvanised steel, with a recessed detail in which the removable UPVC insert clicks into place

	   (= Counteracts horizontal line formation by limiting the penetration of the fabric and facilitates (dis)assembly of the fabric)

	 - Conical fabric tube end pieces (= Compensating for the thicker ends of the rolled-up zipper and thus guaranteeing perfect roll-up of the screen)

	Connect&Go-technology: (Dis)assembly of the fabric set is facilitated by means of the electrical connection: Connect&Go-technology.

	

	Fabric

	All fabrics consist of a single piece of fabric, except when the height is greater than the fabric tube width.

	Confection :

	 - Horizontally

	 - Fixscreen-technology: the vertical borders are equipped with a symmetrical zipper

	   (= This symmetrical shape ensures that the fabric absorbs the wind load well. As a result, the fabric is firmly affixed in both side guiding channels and remains windproof in any position) 

	 - Welding zipper: High-frequency, always on the least visible side. (= Durable and aesthetic adhesion of the zippers to the fabric)

	

	Applicable dimensions of fabrics, see brochure.

	Type of fabric :

	●  Fibre glass fabric (semi-transparent):

	    - Fire resistance: M1 (NFP 92503), C-s3d0 (Euroclass EN 13501-1)

	    - Weight: ± 520-620 g/m², thickness: 0.53-0.80 mm

	    + Crystal window in the full width: Can be integrated if 'Freestanding' F

	●  Polyester fabric (semi-transparent - insect-proof):

	    - Weight: ± 240 g/m²

	

	Weighted bottom bar

	Composition:

	 - Bottom bar: Extruded aluminium, solidly weighted with bars in galvanised steel. (= Facilitates the smooth guiding system and tension of the fabric)

	 - Ballast: Steel bar. The bar is covered with PE foam to prevent contact between the aluminium and steel and to buffer noise

	 - Dimensions and weight of the bottom bar: H 46 mm x D 30 mm (excl. sealing strip) = 0.85 kg/rm

	 - Dimensions and weight of the steel bar: H 30 mm x D 20 mm = 4.7 kg/rm (W = 3120 mm: max. 17 kg), is provided based on the application for ideal guiding system

	Finishing :

	 - The bottom bar disappears completely into the head box

	 - Fitted with UPVC end pieces. Available in 4 colours: black, white, grey and cream

	 - Fitted with a UPVC sealing strip to close off the sill. Available in 2 colours: black and grey.

	

	Colour

	Aluminum profiles (head box, side guiding channels and bottom bar): Powder coated (60-80 µm) or anodised (20 µm) in the same colour as the external joinery.

	Side supporting end caps (cast aluminium): Powder coated in the same colour as the profiles.

	In the case of anodised profiles (head box, side guiding channels and bottom bar), the side supporting end caps are powder coated in the most suitable colour (60-80 µm).

	

	Control

	Electric:

	 - 230 V AC tubular motor, without emergency manual control

	 - 230 V AC tubular motor, with obstacle detection (Detecto) and continuous fabric stretch compensation

	The motor connection is included in the sun protection category and is provided with a uv-resistant cable.

	The electrical connection and all additional wiring are included in the electrical category.

	

	Connect&Go-technology: electrical connection 

	Facilitates quick and easy (dis)assembly of the screen set, IP44 certified.

	When installing the fabric set in the head box, the motor connector moves via the straight guiding system of the corresponding side supporting end piece in the cable connector; both connector clips are fixed into place and form a perfect electrical connection inside the head box.

	

	Renson Connect

	Optional control with Renson smartphone application for iOS and Android, including product details and product-specific tips & tricks in the app.

	

	Warranty and product information via QR code

	10-year warranty on coatings on the aluminium profiles.

	7-year warranty on electronic motors with obstacle detection (Detecto).

	5-year warranty on the windproof-technology if 'Freestanding' F:

	 - Zipper remains in side guiding channel

	 - Optimal adhesion of zipper to fabric

	5-year warranty on defects arising from normal domestic use and regular maintenance.

	5-year warranty on motors.

	5-year warranty on the fabric collection (2-year warranty for Crystal fabric).

	Every individual sun protection product can be identified afterwards and linked to a warranty number or a unique screen ID.

	This identification is done thanks to a QR code, which is placed in an easily accessible location (can be consulted without using extra tools) and can be easily scanned using a smartphone or tablet.

	The essential product details (dimensions, colours, fabric type, motor type, etc.) can be consulted at any time.

	

	Wind class 

	This product meets European standard EN13561.

	Guaranteed up to 60 km/h in closed position in 'Freestanding' F (EN 13561:2004+A1:2008 in accordance with wind class 3). The wind resistance depends on the dimensions and is available upon request.

	Wind tunnel test report by ‘Velux’ (WTT18-002 Fixscreen 100 Slim 2.0): wind resistance guaranteed up to 126 km/h in closed position (tested for a screen of 3,000 mm x 3,000 mm).

	

	Standards and certificates

	This product is manufactured in accordance with: EN 13561 and conforms to and/or has been tested in accordance with these standards.

	Declaration of performance: DoP-2015SC00002.

	AluEco en VMRG Sun protection certificate.

	EU declaration of conformity - In accordance with the following directives:

	 - Machinery Directive 2006/42/EC

	 - Low Voltage Directive 2014/35/EU

	 - EMC Directive 2014/30/EU



