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	Product characteristics

	(text highlighted in red can be deleted depending on your choice)

	

	Installation 

	This product is installed in front of the window with fully finished head box -> Recessed or Surface-mounted:

	The side supporting end caps of the head box, which support the roller mechanism and are equipped with pins, connect the head box to the side guiding channels.

	During the installation of the fabric set (fabric tube + fabric + motor), the electrical connection is made easily via the motor connector.

	170 N/m required construction load on top or behind combined with head box.

	This product can be coupled with the FIXSCREEN 100 Slim IM 7A.

	

	Head box 

	Composition: extruded aluminium.

	Head box design: Square (rectangular).

	Dimensions: 150 mm height and 110 mm depth.

	The product comprises two mitred head boxes, which create a combined head box with an angle of 90° when installed.

	Every head box comprises two fixed profiles and a removable bottom profile.

	Fixed on the perpendicular construction load on top or lying behind,or flat construction.

	

	Side guiding channels 

	Composition:

	The product consists of two parts, each of which is equipped with a side guiding channel. There is no aluminium side guiding channel or cable guiding system in the corner.

	 - Outer profiles: extruded aluminium

	 - 3-piece: u-profile allows for easy disassembly of the fabric set; without complete disassembly of the side guiding channel, without drilling or channelling, which guarantees water and wind proofing

	 - Inner rail:

	    - HPVC plastic (= robust design guarantees high wind guarantees)

	    - Smooth-technology: coextruded, wear-resistant top layer (= Smooth and quiet, long-term durable operation, without additional maintenance)

	    - Neoprene buffer zones (60 mm long) (= Compensate for gusts of wind and contribute to constant fabric tension)

	 - Deep side guiding channel (standard): W 35 mm x D 110 mm, in 3 parts, u-profile; side guiding channel depth = head box depth, equipped with a base plate under 0° or 5° made of fibre glass-reinforced polyamide

	 - Closed side guiding channel: W 35 mm x D 48 mm, in 3 parts; in case used with a self-designed removable finishing, equipped with a base plate under 0° or 5° made of fibre glass-reinforced polyamide

	 - Fixed directly onto the frame/construction. No screws are visible from the façade side

	

	Fabric set

	The product consists out of two fabric tubes that are connected at a 90° angle. The connection is created using hypoid stainless steel gears which are fixed in a corner bracket.

	Composition:

	 - Fabric tube: Galvanised steel, with an integrated recessed fabric groove

	   (= Counteracts horizontal line formation by limiting the penetration of the fabric)

	 - Conical fabric tube end pieces (= Compensating for the thicker ends of the rolled-up zipper and thus guaranteeing perfect roll-up of the screen)

	 - Patented cone shaped fabric tube end pieces and the hypoid gears are fitted to both corner sides

	Connect&Go-technology: (Dis)assembly of the fabric set is facilitated by means of the electrical connection: Connect&Go-technology.

	 - A patented cone shaped fabric tube end piece, the motor slide and the electrical connection are installed on the motor side

	 - A patented cone shaped fabric tube end piece and a bearing slide are installed on the bearing side

	Every fabric set can be disassembled via the removable profile of the head box; the left or right position is determined in this way (cable feed).

	

	Fabric

	The product consists out of two pieces of fabric, where the fabric can be rolled-up and down simultaneously.

	All fabrics consist of a single piece of fabric, except when the height is greater than the fabric tube width.

	Confection :

	 - Horizontally

	 - Fixscreen-technology: the vertical borders are equipped with a symmetrical zipper

	    - The vertical border on one side of each piece of fabric is equipped with a zipper, making the fabric windproof in the side guiding channel

	    - The vertical border at the corner side of each piece of fabric is equipped with a seal strip

	 - Welding zipper: High-frequency, always on the least visible side. (= Durable and aesthetic adhesion of the zippers to the fabric)

	

	Applicable dimensions of fabrics, see brochure.

	Type of fabric :

	●  Fibre glass fabric (semi-transparent):

	    - Fire resistance: M1 (NFP 92503), C-s3d0 (Euroclass EN 13501-1)

	    - Weight: ± 520-620 g/m², thickness: 0.53-0.80 mm

	

	Weighted bottom bar

	Composition:

	The product comprises two mitred bottom bars, which create a combined bottom bar with an angle of 90° when installed.

	Disappears into the head box.

	Each bottom bar is made of a single extruded aluminium profile and is entirely weighted with galvanised steel bars.

	Joint together by means of a corner piece.

	 - Dimensions and weight of the bottom bar: H 46 mm x D 30 mm (excl. sealing strip) = 0.85 kg/rm

	 - Dimensions and weight of the steel bar: H 30 mm x D 20 mm = 4.7 kg/rm

	Finishing :

	 - Fitted with UPVC end pieces. Available in 4 colours: black, white, grey and cream

	 - Fitted with a UPVC sealing strip to close off the sill. Available in 2 colours: black and grey.

	

	Colour

	Aluminum profiles (head box, side guiding channels and bottom bar): Powder coated (60-80 µm) or anodised (20 µm) in the same colour as the external joinery.

	Side supporting end caps (cast aluminium): Powder coated in the same colour as the profiles.

	In the case of anodised profiles (head box, side guiding channels and bottom bar), the side supporting end caps are powder coated in the most suitable colour (60-80 µm).

	

	Control

	Electric:

	A motor is fitted into one of the two parts of the product.

	 - 230 V AC tubular motor, without emergency manual control

	The motor connection is included in the sun protection category and is provided with a uv-resistant cable.

	The electrical connection and all additional wiring are included in the electrical category.

	

	Connect&Go-technology: electrical connection 

	Facilitates quick and easy (dis)assembly of the screen set, IP44 certified.

	When installing the fabric set in the head box, the motor connector moves via the straight guiding system of the corresponding side supporting end piece in the cable connector; both connector clips are fixed into place and form a perfect electrical connection inside the head box.

	

	Renson Connect

	Optional control with Renson smartphone application for iOS and Android, including product details and product-specific tips & tricks in the app.

	

	Warranty and product information via QR code

	10-year warranty on coatings on the aluminium profiles.

	7-year warranty on the windproof-technology:

	5-year warranty on defects arising from normal domestic use and regular maintenance.

	5-year warranty on the electronic control (Somfy automation).

	5-year warranty on motors.

	5-year warranty on the fabric collection.

	Every individual sun protection product can be identified afterwards and linked to a warranty number or a unique screen ID.

	This identification is done thanks to a QR code, which is placed in an easily accessible location (can be consulted without using extra tools) and can be easily scanned using a smartphone or tablet.

	The essential product details (dimensions, colours, fabric type, motor type, etc.) can be consulted at any time.

	

	Wind class 

	Wind tunnel test report by ‘Velux’ (WTT14-001 Panovista): wind guarantee of up to and including 37 km/h in closed position (tested on a 4,000 mm x 4,000 mm x 2,700 mm screen).

	Guaranteed up to 37 km/h in closed position.

	Wind sensor required.

	

	Standards and certificates

	This product is manufactured in accordance with: EN 13561 and conforms to and/or has been tested in accordance with these standards.

	Declaration of performance: DoP-2015SC00004.

	EU declaration of conformity - In accordance with the following directives:

	 - Machinery Directive 2006/42/EC

	 - Low Voltage Directive 2014/35/EU

	 - EMC Directive 2014/30/EU



