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	Product characteristics 

	(text highlighted in red can be deleted depending on your choice)

	

	Installation 

	This product is installed with fully finished head box:

	'Freestanding' F (cannot be coupled) without underlying window.

	 - Installation method 7A (Standard, internal side patio cover or balcony)

	In front of the window -> Recessed.

	 - Installation method 7A (Standard, fabric close to the window)

	Necessary securing for the brackets left and right  independent of installation with or without head box.

	When head box width 3600 mm < 6000 mm, it must be secured once in the middle. When width > 6000 mm, it must be secured twice. In order to avoid bending.

	The head box can be equiped with following options:

	 - With a hook-in profile; hooks into a recess at the back side of the head box, for easy head box securing. Additional installation dimension for hook-in = + 5 mm

	 - With fixation bracket to be fixed on the top of the window frame and specific coupling piece (to be fixed easily on the back side of the head box by means of the rotating profile), for easy head box securing

	 - Without hook-in profile

	The side supporting end caps of the head box, which support the roller mechanism and are equipped with pins, connect the head box to the side guiding channels.

	One side supporting end cap is equipped with the cable connector of the electrical connection.

	During the installation of the fabric set (fabric tube + fabric + motor), the electrical connection is made easily via the motor connector.

	Connect&Go-technology: facilitates quick and easy (dis)assembly of the fabric set.

	The cable feed is located following the choice of installation.

	You can disassemble the fabric set on the side of the removable profile of the head box; the left or right position is determined in this way (cable feed).

	

	Head box 

	Composition: extruded aluminium.

	Head box design: Square (rectangular).

	Dimensions: 180 mm height and 170 mm depth.

	

	Side guiding channels 

	Dimensions: 58 mm width and 40 mm depth

	Composition :

	Are made of extruded aluminium profiles.

	 - In 2 parts: disassembly of the fabric set is possible after disassembly the emovable profile from the side guiding channel

	    - Every side guiding channel is equipped with a UPVC base plate under 0°

	    - Smooth-technology: coextruded, wear resistant top layer (= Smooth and quiet, long-term durable operation, without additional maintenance)

	Installation :

	Fixed directly onto the frame/construction.

	

	Fabric set 

	Composition :

	 - Fabric tube: galvanised steel, with a recessed detail in which the removable UPVC insert clicks into place

	   (= Counteracts horizontal line formation by limiting the penetration of the fabric and facilitates (dis)assembly of the fabric)

	 - Narrowed cone shaped fabric tube end pieces (= Compensating for the thicker ends of the rolled-up zipper and thus guaranteeing perfect roll-up of the screen)

	Connect&Go-technology: (Dis)assembly of the fabric set is facilitated by means of the electrical connection: Connect&Go-technology.

	

	Fabric 

	All fabrics consist of a single piece of fabric, except if the height is greater than the fabric tube width.

	Confection :

	 - Horizontal 

	 - Fixscreen-technology: the vertical borders are equipped with a symmetrical zipper

	   (= This symmetrical shape ensures that the fabric absorbs the wind load well. As a result, the fabric is firmly affixed in both side guiding channels and remains windproof in any position) 

	 - Welding zipper: High-frequency, always on the least visible side. (= Durable and aesthetic adhesion of the zippers to the fabric)

	

	Applicable dimensions of fabrics, see brochure.

	Type of fabric :

	●  Fibre glass fabric (semi-transparent):

	    - Fire resistance: M1 (NFP 92503), C-s3d0 (Euroclass EN 13501-1)

	    - Weight: ± 520-620 g/m², thickness: 0.53-0.80 mm

	

	Weighted bottom bar

	Composition :

	Material: extruded aluminium, weighted with galvanized steel bars.

	 - Dimensions bottom bar: H 60 mm x D 45 mm (excl. sealing strip)

	Finishing :

	 - Welded seam hidden in the bottom bar

	 - Is equipped with black UPVC end pieces

	 - Is equipped with a black UPVC sealing strip to seal off the sill. Available in 2 dimensions: H 7 mm x D 7 mm of H 35 mm x D 31 mm

	 - Easy (dis)assembly of the fabric by a hidden UPVC click profile

	

	Colour 

	Aluminum profiles (head box, side guiding channels and bottom bar): Powder coated (60-80 µm) or anodised (20 µm) in the same colour as the external joinery.

	Side supporting end caps (cast aluminium): Powder coated in the same colour as the profiles.

	In case of anodised profiles (head box, side guiding channels and bottom bar), the side supporting end caps are powder coated in the most suitable colour (60-80 µm).

	

	Control 

	Electrical :

	 - 230 V AC tubular motor, without emergency manual control

	 - 230 V AC tubular motor, with obstacle detection (Detecto) and continuous fabric stretch compensation

	The motor connection is included in the sun protection category and is provided with a UV resistant cable.

	The electrical connection and all additional wiring are included in the electrical category.

	

	Connect&Go-technology: electrical connection 

	Facilitates quick and easy (dis)assembly of the fabric set.

	When installing the fabric set in the head box, the motor connector moves via the straight guiding system of the corresponding side supporting end piece in the cable connector; both connector clips are fixed into place and form a perfect electrical connection inside the head box.

	

	Renson Connect

	Optional control with Renson smartphone application for iOS and Android, including product details and product-specific tips & tricks in the app.

	

	Warranty and product information via QR code

	10-year warranty on coatings on the aluminium profiles.

	7-year warranty on electronic motors with obstacle detection (Detecto).

	7-year warranty on the windproof-technology:

	 - Zipper remains in side guiding channel

	 - Optimal adhesion of zipper to fabric

	5-year warranty on defects arising from normal domestic use and regular maintenance.

	5-year warranty on motors.

	5-year warranty on the fabric collection.

	Every individual sun protection product can be identified afterwards and linked to a warranty number or a unique screen ID.

	This identification is done thanks to a QR code, which is placed in an easily accessible location (can be consulted without using extra tools) and can be easily scanned using a smartphone or tablet.

	The essential product details (dimensions, colours, type of fabric, motor type, etc.) can be consulted at any time.

	

	Wind class 

	This product meets European standard EN13561.

	

	Standards and certificates 

	This product is manufactured in accordance with: EN 13561 and conforms to and/or has been tested in accordance with these standards.



