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	Product characteristics

	(text highlighted in red can be deleted depending on your choice)

	

	Installation of the head box

	This product is installed in front of the window with empty head box and can be completed with the fabric set later on  (=’Fixscreen Ready 100 Slim fabric set’). -> Recessed:

	 - Installation method 7A (Standard, fabric close to the window); this product can be joined to the PANOVISTA

	 - Installation method 7B (Fabric away from the window; cannot be coupled)

	Necessary securing, in order to avoid bending

	To be carried out by means of connection between fixation bracket (to be fixed on the top of the window frame) and specific coupling piece (to be fixed easily on the back of the head box by means of self-tapping screws)

	The side supporting end caps of the head box, which support the roller mechanism and are equipped with pins, connect the head box to the side guiding channels.

	The cable feed is equipped in the head box or is equipped in the side supporting end cap.

	

	Head box 

	The box is finished with a finishing profile.

	Composition: extruded aluminium.

	Head box design: Square (rectangular).

	Dimensions: 150 mm height and 110 mm depth (max. surface 16.8 m²).

	

	Side guiding channels head box

	Composition:

	Fixed profile from the deep side guiding channel (standard): W 35 mm x D 110 mm.

	The side guiding channels are finished with a finishing profile.

	Side guiding channel option:

	 - Deep side guiding channel (standard): W 35 mm x D 110 mm, in 3 parts, u-profile; side guiding channel depth = head box depth, equipped with a base plate under 0° or 5° (only for method 7A) made of fibre glass-reinforced polyamide

	

	Colour

	Aluminum profiles (head box, side guiding channels and bottom bar): Powder coated (60-80 µm) or anodised (20 µm) in the same colour as the external joinery.

	Side supporting end caps (cast aluminium): Powder coated in the same colour as the profiles.

	In the case of anodised profiles (head box, side guiding channels and bottom bar), the side supporting end caps are powder coated in the most suitable colour (60-80 µm).

	

	Control

	Electric:

	 - 230 V AC tubular motor, without emergency manual control

	 - 230 V AC tubular motor, with obstacle detection (Detecto) and continuous fabric stretch compensation

	The motor connection is included in the sun protection category and is provided with a uv-resistant cable.

	The electrical connection and all additional wiring are included in the electrical category.

	

	Connect&Go-technology: electrical connection 

	Facilitates quick and easy (dis)assembly of the screen set, IP44 certified.

	When installing the fabric set in the head box, the motor connector moves via the straight guiding system of the corresponding side supporting end piece in the cable connector; both connector clips are fixed into place and form a perfect electrical connection inside the head box.

	

	Renson Connect

	Optional control with Renson smartphone application for iOS and Android, including product details and product-specific tips & tricks in the app.

	

	Warranty and product information

	10-year warranty on coatings on the aluminium profiles.

	5-year warranty on defects arising from normal domestic use and regular maintenance.

	Every individual sun protection product can be identified afterwards and linked to a warranty number or a unique screen ID.

	

	Wind class 

	This product meets European standard EN13561.

	Guaranteed up to 130 km/h in closed position (EN 13561:2004+A1:2008 in accordance with wind class 3). The wind resistance depends on the dimensions and is available upon request.

	Wind tunnel test report by ‘Velux’ (WTT18-002 Fixscreen 100 Slim 2.0): wind resistance guaranteed up to 126 km/h in closed position (tested for a screen of 3,000 mm x 3,000 mm).

	

	Standards and certificates

	This product is manufactured in accordance with: EN 13561 and conforms to and/or has been tested in accordance with these standards.

	Declaration of performance: DoP-2015SC00002.

	AluEco en VMRG Sun protection certificate.

	EU declaration of conformity - In accordance with the following directives:

	 - Machinery Directive 2006/42/EC

	 - Low Voltage Directive 2014/35/EU

	 - EMC Directive 2014/30/EU



