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	Product characteristics 

	(text highlighted in red can be deleted depending on your choice)

	

	Installation 

	This product is installed in front of the window with fully finished headbox -> Recessed or Surface mounted:

	 - Installation method 7A (Standard, fabric away from the window; cannot be coupled)

	 - Installation method 7B (Fabric away from the window; cannot be coupled)

	The headbox and side guiding channels can be installed in installation method  ‘A’ as ‘B’, to determine in the factory or on site.

	The securing of the headbox against the construction is not necessary.

	The side supporting end caps of the headbox, which support the roller mechanism and are equipped with pins, connect the headbox to the side guiding channels.

	The side supporting end cap is equipped with a ‘Click & Safe’ slide, for simple (dis)assembly of the fabric set.

	The cable feed is located following the choice of installation.

	

	Headbox 

	Composition: extruded aluminium.

	Headbox design: Square (rectangular) beveled on one side.

	Dimensions: 90 mm height and 90 mm depth (max. surface 7.8 m²).

	

	Side guiding channels 

	Composition :

	Fixed profile from the deep side guiding channel (standard): W 35 mm x D 90 mm.

	Fixed profile from the narrow side guiding channel (standard): W 35 mm x D 50 mm.

	The side guiding channels are finished with a removable profile.

	 - Outer profiles: extruded aluminium

	 - Inner rail :

	    - HPVC plastic (= robust design guarantees high wind guarantees)

	    - Smooth-technology: coextruded, wear resistant top layer (= Smooth and quiet, long-term durable operation, without additional maintenance)

	    - Neoprene buffer zones (60 mm long) (= Compensate for gusts of wind and contribute to constant fabric tension)

	    - Flush-mounted in 2 parts side guiding channel, reducing visibility

	Side guiding channel option:

	 - Deep side guiding channel (in 2 parts)

	 - Narrow side guiding channel (in 2 parts)

	 - Equipped with a black base plate under 0° or 5°

	 - Fixed directly onto the frame/construction. No screws are visible from the facade side

	

	Fabric set 

	Composition :

	 - Fabric tube: aluminium, with an integrated recessed fabric groove

	   (= Counteracts horizontal line formation by limiting the penetration of the fabric and facilitates (dis)assembly of the fabric)

	 - Narrowed cone shaped fabric tube end pieces (= Compensating for the thicker ends of the rolled-up zipper and thus guaranteeing perfect roll-up of the screen)

	Click&Safe-technology: The fabric set can be clicked into the headbox without screws so that the installer has his hands free to safely complete the installation.

	

	Fabric 

	All fabrics consist of a single piece of fabric, except if the height is greater than the fabric tube width.

	Confection :

	 - Horizontal 

	 - Fixscreen-technology: the vertical borders are equipped with a symmetrical zipper

	   (= This symmetrical shape ensures that the fabric absorbs the wind load well. As a result, the fabric is firmly affixed in both side guiding channels and remains windproof in any position) 

	 - Welding zipper: High-frequency, always on the least visible side. (= Durable and aesthetic adhesion of the zippers to the fabric)

	

	Applicable dimensions of fabrics, see brochure.

	Type of fabric :

	●  Fibre glass fabric (semi-transparent):

	    - Fire resistance: M1 (NFP 92503), C-s3d0 (Euroclass EN 13501-1)

	    - Weight: ± 520-620 g/m², thickness: 0.53-0.80 mm

	●  Fibre glass fabric (blackout):

	    - Fire resistance: M1 (NFP 92503)

	    - Weight: ± 660 g/m², thickness: 0.75 mm

	

	Weighted bottom bar

	Composition :

	 - Bottom bar: Extruded aluminium, solidly weighted with bars in galvanised steel. (= Facilitates the smooth guiding system and tension of the fabric)

	 - Ballast: Steel bar. The bar is covered with PE foam to prevent contact between the aluminium and steel and to buffer noise

	 - Dimensions bottom bar: H 47 mm x D 30 mm

	Finishing :

	 - The bottom bar disappears partially into the headbox

	 - Is equipped with black UPVC end pieces

	 - Is equipped with a black UPVC sealing strip to seal off the sill

	

	Colour 

	Aluminum profiles (headbox, side guiding channels and bottom bar): Powder coated (60-80 µm) in the same colour as the external joinery.

	Side supporting end caps (cast aluminium): Powder coated in the same colour as the profiles.

	

	Control 

	Electrical :

	 - 230 V AC tubular motor, without emergency manual control

	 - 230 V AC tubular motor, with obstacle detection (Detecto) and continuous fabric stretch compensation

	The motor connection is included in the sun protection category.

	The electrical connection and all additional wiring are included in the electrical category.

	

	

	Warranty and product information via QR code

	10-year warranty on coatings on the aluminium profiles.

	7-year warranty on electronic motors with obstacle detection (Detecto).

	7-year warranty on the windproof-technology:

	 - Zipper remains in side guiding channel

	 - Optimal adhesion of zipper to fabric

	5-year warranty on defects arising from normal domestic use and regular maintenance.

	5-year warranty on (Renson) motors.

	5-year warranty on the fabric collection.

	Every individual sun protection product can be identified afterwards and linked to a warranty number or a unique screen ID.

	This identification is done thanks to a QR code, which is placed in an easily accessible location (can be consulted without using extra tools) and can be easily scanned using a smartphone or tablet.

	The essential product details (dimensions, colours, type of fabric, motor type, etc.) can be consulted at any time.

	

	Wind class 

	This product meets European standard EN13561.

	Guaranteed up to 130 km/h in closed position (EN 13561:2004+A1:2008 conform wind class 3).

	

	Standards and certificates 

	This product is manufactured in accordance with: EN 13561 and conforms to and/or has been tested in accordance with these standards.

	Declaration of performance: DoP-2015SC00002.

	AluEco en VMRG Sun protection certificate.

	EU declaration of conformity - In accordance with the following directives:

	 - Machinery Directive 2006/42/EC

	 - Low Voltage Directive 2014/35/EU

	 - EMC Directive 2014/30/EU



