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	Product characteristics

	(text highlighted in red can be deleted depending on your choice)

	

	Installation 

	This product is installed on a closed structure (e.g. a skylight) with or without mounting bases.

	Only top-bottom installation is possible.

	The inclination angle may vary between 0° and 90°. The usage of a type of fabric is defined in function of the inclination angle.

	

	Head box 

	Dimensions: 230 mm height and 140 mm depth

	Profiles are made of extruded aluminium.

	

	Side guiding channels 

	Are made of 1 extruded aluminum profiles.

	Dimensions :

	    - Side guiding channel: W 41.5 mm x D 67 mm

	The side guiding channels are equipped with cavities in which the belt and the pulley wheel of the tension system is located. The lower cavity is sealed off over the complete length by means of an ornamental strip.

	    - Coupling side guiding channel: W 84 mm x D 67 mm

	

	Fabric tube 

	Made of galvanised steel.

	Is equipped with a motor tube which is part of the tension system.

	You can disassemble the fabric set on the side of the removable profile of the head box; the left or right position is determined in this way (cable feed).

	

	Fabric

	●  Polyester fabric (semi-transparent):

	    - Fire resistance: M1 (NFP 92503), B-s2d0 (Euroclass EN 13501-1)

	    - Weight: ± 380-420 g/m², thickness: 0.43-0.45 mm

	    - All fabrics consist of a single piece of fabric, except when the projection size is greater than the fabric tube width

	    - The fabrics are manufactured horizontally

	    - The vertical borders not welded, bottom and top side welded at high frequency

	

	Bottom bar 

	Is made of 1 extruded aluminium profile.

	

	Tension system 

	The pre-tension is built by means of springs, located on top of the motor tube. This motor tube is located in the fabric tube.

	The number of springs can vary from 2 to 4 pieces depending on the width of the product.

	The system is tensioned using a permanently pre-tensioned Aramide/Kevlar-belt.

	

	Colour

	All visible aluminium profiles (head box, side guiding channels and bottom bar): Powder coated (60-80 µm) in the same colour or anodised (20 µm), as the external joinery.

	The side supporting end caps (cast aluminium): Powder coated (60-80 µm) in the same colour as the profiles.

	For anodised profiles, the side supporting end caps are powder coated in MAT 9006 (head box, side guiding channels and bottom bar).

	

	Control

	Electrical: by means of 230 V AC tubular motor, without emergency manual control

	The motor connection is included in the sun protection category.

	Uv-resistant cable included.

	The electrical connection and all additional wiring are included in the electrical category.

	

	Warranty   

	10-year warranty on coatings on the aluminium profiles.

	5-year warranty on defects arising from normal domestic use and regular maintenance.

	5-year warranty on the electronic control (Somfy automation).

	5-year warranty on the fabric collection.

	

	Wind class 

	⌂ (EN 13561:2004+A1:2008 conform wind class 3).

	

	Standards and certificates

	⌂ This product is manufactured in accordance with: EN 13561 and conforms to and/or has been tested in accordance with these standards

	    - Declaration of performance: DoP-201409-F006



