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	Product characteristics 

	(text highlighted in red can be deleted depending on your choice)

	

	Installation 

	This product is installed onto the VELUX Modular Skylights using mounting bases.

	This sun protection is installed on the fixed modules of the VELUX Modular Skylight construction.

	One or more comfort ventilation modules (open system) or smoke extraction module can be equipped with sun protection, if installed between two fixed modules.

	Top-bottom installation (decending). The inclination angle may vary between 0° and 90°. The usage of a type of fabric is defined in function of the inclination angle.

	The height of the mounting bases depends on the selected VELUX ventilation modules:

	    - In case of the combination 'Fixed modules' and 'Comfort Ventilation module(s)' (open system): Height = 80 mm

	    - In case of the combination 'Fixed modules' and 'Smoke Extraction module(s)': Height = 160 mm

	

	Head box 

	Dimensions: 105 mm height and 100 mm depth

	Profiles are made of extruded aluminium.

	

	Side guiding channels 

	Are made of 2 extruded aluminum profiles.

	Dimensions :

	    - Side guiding channel: W 58 mm x D 48 mm, in 2 parts

	    - Side guiding channel: W 58 mm x D 48 mm

	Each side guiding channel has an integrated UPVC inner rail with a co-extruded, wear resistant top layer to ensure smooth and silent functioning.

	The HPVC inner rail is equipped with 2 S profiles on each side, to compensate heavy wind loads.

	

	Fabric tube 

	Made of galvanised steel.

	An integrated recessed fabric groove limits compression of the fabric loop.

	Is equipped with patented cone shaped fabric tube end pieces to compensate the thicker ends of the zipper.

	They also contain a cord disk to roll up the tension cord.

	You can disassemble the fabric set on the side of the removable profile of the head box; the left or right position is determined in this way (cable feed).

	

	Fabric 

	All fabrics consist of a single piece of fabric, except if the height is greater than the fabric tube width.

	The fabrics are confectionated horizontally.

	The vertical borders are equipped with a zipper to keep the fabric firmly (windproof) in the side guiding channel.

	The zipper is welded at high frequency, always on the least visible side.

	●  Polyester fabric (semi-transparent):

	    - Fire resistance: M1 (NFP 92503), B-s2d0 (Euroclass EN 13501-1)

	    - Weight: ± 380-420 g/m², thickness: 0.43-0.45 mm

	

	Bottom bar 

	Is made of 2 extruded aluminum profiles.

	    - Dimensions bottom bar: H 90 mm x D 50 mm (excl. sealing strip)

	    - Option: dimensions bottom bar: H 60 mm x D 40 mm (excl. sealing strip) if total width of Topfix ≤ 3,000 mm (available untill end of stock)

	The tension system is concealed in the bottom bar. To reduce contact noise between the pull spring and the aluminium bottom bar, the internal side of the aluminium profile has an adhered noise reduction strip.

	Is equipped with UPVC end pieces. Available in four colours: black, white, grey and cream

	Is equipped with a UPVC sealing strip to seal off the sill. Available in two colours: black and grey

	

	Tension system 

	The revolutionary system pretensions the cord by means of springs located in the bottom bar.

	The tension system is unique in combination with our technology. This ensures a windproof screen in any position.

	

	Colour 

	All visible aluminium profiles (head box, side guiding channels and bottom bar): Powder coated (60-80 µm) in the same colour or anodised (20 µm), as the external joinery.

	The side supporting end caps (cast aluminium): Powder coated (60-80 µm) in the same colour as the profiles.

	For anodised profiles, the side supporting end caps are powder coated in MAT 9006 (head box, side guiding channels and bottom bar).

	

	Control 

	Motor type depends on the type of ventilation applied:

	    - In combination with 'Fixed modules' and 'Smoke Extraction module(s)': by 24 V DC tubular motor, without emergency manual control.

	    - In combination with 'Fixed modules' and 'Comfort Ventilation module(s)' (open system): by 230 V AC tubular motor with Standard Motor Interface, without emergency manual control or by 24 V DC tubular motor, without emergency manual control.

	    - In combination only with 'Fixed modules': by 230 V AC tubular motor, without emergency manual control.

	UV resistant cable included.

	

	Electrical connection 

	The electrical connection and all additional wiring are included in the electrical category. These parts must be provided by the M&E engineer on site and are not included in the sun protection category.

	A distribution box must be installed to ensure a correct electrical connection between the VELUX VMS and the Topfix VMS.

	Cables can be conducted in the gutter of the VELUX VMS using a waterproof cable feed with adaptive metal sheet thickness of the gutter.

	A special VELUX approved protocol, is integrated in the Building Management System (BMS).

	    - In case of 230 V AC tubular motor with Standard Motor Interface -> protocol needs to be integrated within the Building Management System (BMS)

	    - In case of 24 V DC tubular motor -> to be realized with the Windowmaster FlexiSmoke module (or equivalent)

	The Building Management System is not part of the sun protection category.

	

	Warranty 

	10-year warranty on coatings on the aluminium profiles.

	7-year warranty on the windproof-technology:

	    - Zipper remains in side guiding channel

	    - Adhesion of zipper to fabric

	5-year warranty on defects arising from normal domestic use and regular maintenance.

	5-year warranty on the electronic control (Somfy automation).

	5-year warranty on the fabric collection.

	Every individual sun protection product can be identified afterwards and linked to a warranty number or a unique screen ID.

	This identification occurs via a QR code, which is placed within reach (without the use of tools) and easily scannable with a smartphone.

	The essential product details (dimensions, colours, type of fabric, motor type, etc.) can be consulted at any time.

	

	Wind class 

	⌂ Guaranteed up to 120 km/h in closed position if H (height of the mounting bases) = 80 mm (EN 13561:2004+A1:2008 conform wind class 3)*.

	    * Wind tunnel test report 'Von Karman Institute' (n° EAR0852 - 2009-07) (W 2,000 mm x P 2,000 mm)

	⌂ Guaranteed up to 80 km/h in closed position if H (height of the mounting bases) = 160 mm (EN 13561:2004+A1:2008 conform wind class 3).

	

	Standards and certificates 

	⌂ This product is manufactured in accordance with: EN 13561 and conforms to and/or has been tested in accordance with these standards

	References and certificates:

	    - Declaration of performance: DoP-201409-F006



